PROTECTOR DE MOTOR ADAPTABLE A SUZUKI GSXR1000 09’-14’
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CRASH PADS ADAPTABLE TO SUZUKI GSXR1000 09’-14’
REF:5295
INSTRUCCIONES DE MONTAJE  

Desmontar los laterales del carenado. Desmontar los tornillos de sujeción del chasis al motor en el punto marcado en la fotografía (y lado contrario). Montar los protectores en el lado correspondiente según el croquis adjunto. Una vez apretado colocar las tapas.

INSTRUCTIONS TO ASSEMBLE

Remove the side bodyworks . Remove the fasteners that subject the chassis to the engine, on the point marked below (and the opposite side). Mount the protectors on each own side as the figure below shows. Tight the set, and place the caps.
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           MATERIAL SUMINISTRADO / MATERIAL SUPPLIED
	POSICIÓN
	DENOMINACIÓN
	CANTIDAD

	1
	Juego de tapas
	Caps set
	2

	2
	Tornillo M10/150X80 DIN912
	DIN912 M10/150X80 fastener
	2

	3
	Arandela (20ext.(10int x2 DIN125/A
	(20ext.(10int x2 washer DIN125/A
	2

	4
	Protector Nylon
	Nylon protector
	2

	5
	Casquillo aluminio 
	Aluminium cylinder 
	2

	6
	Desplazador metálico l/derecho
	Offset  right hand side
	1

	7
	Desplazador metálico l/izquierdo
	Offset left hand side
	1

	8
	Tuerca M10/150 DIN6923
	M10/150 DIN6923
	2

	9
	Tornillo M10/125X60 DIN912
	DIN912 M10/125X60 fastener
	2
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EL MONTAJE DE LOS PROTECTORES DE MOTOR NO GARANTIZAN UNA PROTECCION INTEGRAL EN CASO DE CAIDAS. MOTOPLASTIC-PUIG DECLINA TODA RESPONSABILIDAD EN CASO DE DETERIODO DE LA MOTOCICLETA.

THE USE OF CRASH PADS DO NOT GUARANTEE A FULL PROTECTION IN CASE OF ACCIDENT. MOTOPLASTIC-PUIG DECLINE ANY RESPONSIBILITY IN CASE OF MOTORCYCLE DAMAGE.


