Between 2009 and 2026, Harley-Davidson Touring models use 5 distinct OEM front brake rotor fitments.
Fitment on modern Harley Touring bikes depends heavily on both the rotor diameter and the wheel mounting configuration (traditional hub-mount vs. spoke-mount).
The 5 Touring Front Rotor Fitments
	Fitment Type
	Rotor Diameter
	Mounting Pattern / Type
	Common Models & Years

	1. Standard 5-Bolt Hub-Mount
	11.8" (300 mm)
	5-bolt pattern on a 3.25" bolt circle (2.22" center bore)
	2009–2023 Standard Touring models (Electra Glide, Road King, Street Glide/Road Glide with cast/laced wheels, Talon wheels); carried over on select models like Road King Special.

	2. Enforcer / Prodigy Spoke-Mount
	11.8" (300 mm)
	5-bolt perimeter/spoke-mount pattern (larger center opening, bolts to wheel spokes)
	2014–2023 Street Glide (FLHX) & Road Glide (FLTRX) equipped from the factory with Enforcer, Impeller, or Prodigy wheels.

	3. 7-Bolt Agitator Mount
	11.8" (300 mm)
	Proprietary 7-bolt hub/spoke pattern
	2010–2023 Select CVO models and factory accessory wheels (Agitator, Chisel, and Slicer wheels).

	4. Standard Spoke-Mount (Rushmore Refresh)
	12.6" (320 mm)
	5-bolt spoke-mounted floating rotor
	2024–2026 Standard Touring redesigns (all-new 2024+ Street Glide & Road Glide) and 2023.5 CVO Street Glide / Road Glide.

	5. Hub-Mount (CVO / ST Radial)
	12.6" (320 mm)
	5-bolt hub-mounted pattern (similar hub PCD, enlarged 320 mm diameter)
	2023–2026 CVO Street Glide, CVO Road Glide, and CVO Road Glide ST models with Brembo radial calipers.


Practical Fitment Rules to Keep in Mind
· Rotor Diameter: Touring bikes strictly used 11.8" (300 mm) front discs from 2008 through 2023. Starting with the major redesign in late 2023/2024, the platform upgraded to larger 12.6" (320 mm) rotors paired with updated Brembo caliper geometry. 
· Wheel Swaps (Hub vs. Spoke Mount): Between 2014 and 2023, wheels like the Enforcer or Prodigy bolted the rotor directly into the wheel spokes rather than the center hub. If swapping an Enforcer wheel onto a 2009–2013 bike, you must use the Enforcer-specific spoke-mounted rotors (or an aftermarket hub conversion adapter). 

